Product program / Amplifier / Mixer Amplifier

A-1806    ER

Mixer power amplifier, 8 inputs including  three balanced microphone inputs, input no. 1 with priority override circuit with pre-chime (1-2-sound, 4 sound) via optional combined XLR/ phone jack or DIN socket, the other two with combined XLR/ phone jack, three recording inputs, two with two RCA jacks each and one with combined XLR/ phone jack, recording connection with two RCA jacks for recording devices, two line level outputs, telephone and emergency inputs with control inputs via screw terminals, automatic power-on in emergency case, as well as remote switch-on of booster amplifier, speaker connection by means of screw terminals, 24V-emergency DC input, bass and treble controls, master volume control, designed  as a desk top unit it can also be installed by means of optional brackets MB-25 B in a 19-inch rack cabinet occupying 2 units height. 3 priorities: 1. emergency, 2. phone, 3. remote microphone (MIC 1), two switchable speaker zones, a speaker direct output, indicators for output level, range, power, emergency and telephone; control outputs (screw terminals) for remote power-on of booster amplifiers and activation of emergency operation, rear-side mounted level control for pre-chime, emergency and telephone input as well as music output, optional cover for the master control to protect against accidental or deliberate alteration.