Product program / Amplifier / Mixer Amplifier

A-3212DZ-EB 1CE

The amplifier shall be suited for broadcasting, paging or background music. It shall be highly durably, highly reliable and have a high performance. It shall contain a mute function, a independent input volume control and master volume control. It shall contain an independent tone control of boost and cut type for both high and low frequency. It shall support at least one phantom power interface for microphones. A current limiter circuitry shall protect transistors and a thermal protection circuitry shall prevent a failure due to overheat. All Microphone Inputs shall be electronically-balanced. The amplifier shall contain a zone selector. The amplifier shall have indicators to display its status. The speaker output shall have a constant voltage distribution system (100 V) &amp; low impedance (4 Ω). It shall have a all call knob which activates all zone terminals. It shall contain bass and treble control. It shall have at least 4 mic, 2 aux and priority input. It shall contain a speaker output terminal, a direct line -, zone selection- and record output.
<ul>
<li>Rated output: Min. 120 W</li>
<li>S/N ratio: Min. 60 dB</li>
<li>Operating temperature: Max. 0 °C to min. 40 °C</li>
<li>Frequency response: Max. 50 - min. 20000 Hz</li>
<li>Weight: Max. 5 kg</li>
</ul>