Product program / Amplifier / Mixer Amplifier

A-3524D     4CE

<div>The mixer power amplifier shall operate on AC mains power, and shall control and mix 4 electronically-balanced (2 MIC/Line selectable removable terminal block (5 pins) or Ø6.3 mm phone jack (2p), 1 electronically- balanced Ø6.3 mm phone jack (2p) and 1 MIC/Line selectable Ø6.3 mm phone jack (2p), 1 unbalanced RCA pin jack (x2) and 1 unbalanced PWR AMP IN RCA pin jack. 
Speaker outputs shall be Low impedance (8 – 16 Ω) or high impedance (DIRECT, ZONE 1/ZONE 2: 100V/total 170 Ω) removable terminal block (6 pins). REC Out shall be unbalanced RCA pin jack and LINE out shall be 2 unbalanced RCA pin jacks.
Control Outputs power remote, emergency out and zone control out shall be provided via removable terminal blocks (4 pins).
The amplifier shall meet the following performance criteria: Power output shall be 240 W at less than 1% THD (at 1 kHz, 1/3 rated power). Frequency response shall be 50 Hz to 20 kHz (+/-3 dB), with an S/N ratio of over 88 dB (Master Volume: Min) or 76 dB (Master Volume: max) or 55 dB (Input 1- 4) or 72 dB (Input 5). 
Bass Tone Control shall be +/-10 dB at 100 Hz, and Treble Tone Control shall be +/-10 dB at 10 kHz. 5-point LED outout level meter, Power, priority, emergency, thermal protection, over current protection, zone 1 and zone 2 indicators shall be provided. The panel shall be ABS black resin, and the case black steel plate. Dimensions shall be 420 (W) x 96.1 (H) x 313.1 (D) mm and weight is 4.9 kg.&nbsp;</div><div>The mixer power amplifier shall be TOA model A-3524D.</div>