Product program / Mixer / Modules

AN-001T

Input module with 2 channels for ambient noise-controlled volume control. Connection of two symmetrical sensors and two 3-pin detachable screw connectors. Switchable phantom power for microphones.