Product program / Accessories / Attenuator

ATT-100VI

<span lang="EN-GB">Attenuator card with transformer for the floating adjustment of 100-Volt signals to line level. The attenuation is customisable by adding resistors.</span>
<p class="MsoNormal"><span lang="EN-GB"><span lang="EN-GB">&nbsp;</span></span></p>
<p class="MsoNormal"><span lang="EN-GB">Frequency response (typ.): <span>&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;</span> 50 Hz... 20 kHz (0/-3 dB)</span></p>
<p class="MsoNormal"><span lang="EN-GB">Input voltage: <span>&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;</span> 100 V ~.</span></p>
<p class="MsoNormal"><span lang="EN-GB">Output voltage: <span>&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;</span> 1.23 V ~.</span></p>
<p class="MsoNormal"><span lang="EN-GB">Load impedance: <span>&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;</span> min 10 kOhm</span></p>