Product program / Loudspeaker / Wall

BS-1015BSW

The speaker shall be a High-quality 2-way bass type reflex fitted with a 12cm cone woofer and a 2.5cm dome tweeter speaker suitable for wall or ceiling mounting. Fire-resistant terminal block made of steatite, thermal fuse with blowing temperature of 84°C, internal cables with flame-resistant insulation. Fire Rated Cable can be directly connected to the speaker via 20mm cable glands. The speaker shall be certified according to EN 54-24: 2008 with CPD Number 0359-CPD-0105. Certified according to ISO 7240-24: 2010, Complies to BS-5839-8: 2013 14.8.
The speaker shall include a transformer having multiple taps (5W, 10W, 15W) at 100V adjustable via rotary switch. The output sound pressure level at a distance of 1m with a 1W input level applied shall be 90 dB SPL. The speaker shall have a frequency response of 80 – 20,000Hz (peak -20dB). Ingress Protection, IP33C. The speaker Grill shall be constructed of surface treated steel plate and the cabinet shall be constructed of ABS resin. The speaker shall be available in white or black color. The unit shall have dimensions of 196 (W) × 290 (H) × 180 (D) mm, and a weight of 2.5 kg.

The speaker shall be TOA model BS-1015BSW.