Product program / Loudspeaker / Wall

BS-1030B  EU

Speaker box with elegant softline design fits into modern architecture. High quality 2-way speaker in a bass reflex enclosure suitable for flush-mounting/ surface-mounting wall/ceiling speaker with optional bracket or on an optional floor stand, including 100V-transformer, 12 cm cone Woofer and 2.5 cm dome tweeter designed for both music reproduction and high intelligibility, rotary switch for power adjustment including low impedance selection on the rear. Low resonance ABS enclosure with removable metal grille in the same color as the body , with U-brackets for tilt and pan.