Product program / Loudspeaker / Wall

BS-4W

The splash proof loudspeaker systems shall incorporate a single 10cm (4”) full range plastic type transducer. The unit is contained in a closed weatherproof unit, sealed against ingress of water meeting the requirements for IPX2 standards for water protection. Included shall be a 360&deg; rotatable bracket.
The unit shall have a smooth frequency response between 100 Hz to 12 kHz measured on axis. The loudspeaker shall produce a Sound Pressure Level (SPL) of 87 dB on axis at 1 meter with a power input of 1 watt and shall be capable of producing 5 watts of power. The unit shall include an enclosed 5 watt/100 line transformer with cable entry fixed at the rear of the unit.
The splash proof loudspeaker shall operate in temperature conditions of between -20 ℃ to + 55 ℃ (-4 &deg;F to 131 &deg;F)
The unit construction shall be polypropylene, grey. Grille: aluminium punch net, silver grey. Mounting bracket: Rolled steel plate, grey. Dimensions shall be 196 (W) × 177 (H) × 160 (D) mm (7.72" × 6.97" × 6.3") weighing 1.5 kg (3.31 lb.)