Product program / Loudspeaker / Wall

BS-633A

The speaker shall be a 5" (12cm) cone-type speaker suitable for wall mounting. Cable connection shall be by means of a push-in connector (bridging terminal). The speaker shall include a transformer having multiple taps (1W, 3W, 6W at 100V and 0.5W, 1.5W, 3W at 70V) adjustable. The output sound pressure level at a distance of 1m with a 1W input level applied shall be 91 dB SPL. The speaker shall have a frequency response of 120 – 15,000Hz (-20dB). The speaker enclosure shall be constructed of ABS resin. The speaker shall be available in off-white colour. The unit shall have dimensions of 173 (W) x 195 (H) x 101 (D) mm (6.81” x 7.68” x 3.98”), and a weight of 780g (1.72 lbs.).
The speaker shall be a TOA model BS-633A.