Product program / Loudspeaker / Wall

BS-680F

The speaker shall be a 16cm (6") double cone-type box speaker suitable for wall mounting. Cable connection shall be by means of a push-in connector bridging terminal. The speaker shall be able to be quickly and easily installed in either a horizontal or a vertical orientation. Both wall and in-wall mounting shall be possible. The speaker shall include a transformer having multiple taps (0.8W, 1.5W, 3W, 6W at 100V and 0.4W, 0.8W, 1.5W, 3W at 70V) adjustable. The sensitivity at a distance of 1m with a 1W input level applied shall be 94dB. The speaker shall have a frequency response of 150Hz – 20kHz (-20dB).
The speaker baffle and cabinet shall be constructed of steel plate. The grille shall be surface-treated steel plate net. The speaker shall be available in off-white color. The unit shall have dimensions of 310 (W) x 190 (H) x 87.2 (D) mm (12.2" x 7.48" x 3.43"), and a weight of 2.6 kg (5.73 lbs.).
The speaker shall be a TOA model BS-680F.