Product program / Mixer / Accessory

D-2012C   CE

Remote control console in 19-inch version, 12 smooth-running&nbsp; 100 mm motor faders with 8 rotary encoders to the continuous volume of 12 inputs and 8 outputs, 8 push buttons with integrated LEDs programmable functions such as preset option, input channel selection, channel switch / switch off and gradually increase the volume / lower, light-emitting diode display of preset selection, input channel selection and channel, switched on or off. Level indicated by the LED row for all control. Switch to the remote activation of a single digital mixer or of the complete system. Equipped with a stereo RCA line input to the audio input on the monitor bus. Stereo headphone output signal control in the overall system. Connector RS-232 for parameterization, remote control over media control, to service purposes and to the firmware update. 10BASE-t/100BASE-TX RJ-45 network connector for system connection via TCP/IP. Symmetrical monitor bus with a send and a return channel.

Separate table enclosure with padded wrist rest optional. Manufacturer strangers adapted or consoles created by special are disallowed due to interchangeability, replenishment and service. The console should contain no internal audio signal processing on the basis of simple cabling and interference.