Product program / Mixer / Modules

D-984VC

Remote control module with 8 RJ45 Sockets for 8 inputs, 8 floating control outputs and 20 volume control inputs. 
Control inputs to select presets, volume adjustment, switching on and off of the inputs or outputs and selection of stereo inputs, free programmable via software.
Remote continuous volume control DC (VCA) of 12 input and 8 output channels, simple connection of potentiometers and faders without external power supply, as power supply is provided by the RJ45 jacks.
Status information can be removed simultaneously the control outputs for the functions of the control inputs as feedback and for interfacing to other systems.