Product program / Mixer / Processor Unit

DP-K1     CE301

Modular digital signal processor with anti-response function for up to 8 audio inputs and 8 outputs. Through the feedback function is achieved depending on the acoustic environment a much clearer sound and thus increases the intelligibility. Automatic measurement of the room up to 8 measurement locations with analysis of the critical room resonances. Up to 8 zones can be individually adjusted.
Each signal path has 18 filter, of which 12 are free configurable and programmable from the following types: parametric EQ, high, low and all pass filter, notch filters, shelving filters for bass and treble, CD Horn equalization.
Other DSP functions per signal path: mixing matrix, 2 level controls, gain, phase reversal, 2 squelch, delay up to 682 ms, 2 compressors, 2-, 3-, 4-way crossover with run-time correction (alignment).
8 configuration presets storable in the device and accessible on the unit or by remote control. Variable access lock with password protection programmable for the software.
All inputs and outputs with led signal indicator. 
6 Slots for various analog and digital input and output modules, a socket for remote control modules configuration selection and volume adjustment. Matching optional modules for analog microphone and line level inputs, as well as for the digital formats (24-bit) AES/EBU and SPDIF.
Including control software for PC/laptop on Windows® interface. Creation of the configuration online and offline via Ethernet interface in real time. Simple firmware update. 

®: brands registered by Microsoft Corporation