Product program / Loudspeaker / Wall

F-1000BTWPEB-Q

Weatherproof, compact 2-way design speaker in an attractive housing made of impact-resistant polystyrene with steel mesh panel. The extremely stiff construction of the housing achieved by the housing material and its shape minimizes the resonance, thereby allowing a clear reproduction. Tweeter with octagon horn for improved sound dispersion characteristics compared to a standard CD horn. Rear rotary switch for power adjustment.
Including swivel and tilt wall / ceiling mount, which can be attached to the bottom and back of the speaker.

Rated power: 15 W

Tappings 100V: 15/5/3/1 W

Tappings 70V: 15 / 7.5 / 2.5 / 1.5 / 0.5 W

Frequency range: 85 - 20000 Hz (-10 dB)

SPL: 87 dB (1W, 1m)

Dispersion angle (-6 dB): 90 ° x 90 °

Degree of protection: IPX4 

Type (EN 54-24):	A

Dimensions (W x H x D): 130 x 202 x 131 mm

Weight: 2 kg (incl. bracket)
Color: black

Brand: TOA

Type: F-1000BTWPEB-Q

Number of certificate:	1138/CPD/0282

Number of notified body:	1138