Product program / Loudspeaker / Wall

F-1000BT

The speaker shall be a two-way bass reflex enclosure suitable for ceiling or wall mounting. The low frequency component shall be a10 cm (4") cone-type woofer. The high frequency component shall be a balanced dome tweeter. For clear, wide-area sound coverage, the speaker shall 90° (H) x 90° (V) wide dispersion-angle high frequency horn.
The rated input shall be 15 W. The speaker shall include a transformer having multiple taps (8ohm, 1 W, 3 W, 5 W, 15 W at 100 V and 0.5 W, 1.5 W, 2.5 W, 7.5 W, 5 W at 70 V) adjustable via the rear of the enclosure. The sensitivity at a distance of 1m with a 1 W input level applied shall be 87 dB. The speaker shall have a frequency response of 85 – 20kHz.
The speaker enclosure shall be constructed of HIPS resin. The speaker shall be available in white or black, and also be repaintable. The grille shall be a punched net, surface-treated steel plate. Brackets for speakerstand, wall and ceiling installation shall be included. There shall be also optionally available brackets for more demanding installations.
The unit shall be compact and lightweight with dimensions of 130 x 202 x 131 mm (5.12" x 7.95" x 5.16") and a weight of 1.8 kg (3.97 lbs.).

The speaker shall be a TOA model F-1000BT/F-1000WT.
The board hanger bracket shall be the HY-BH10B.
The ceiling mount bracket shall be the HY-CM10B/HY-CM10W.
The cluster bracket shall be the HY-CL10B.