Product program / Loudspeaker / Wall

F-1000B

The speaker shall be a two-way bass reflex enclosure suitable for ceiling or wall mounting. The low frequency component shall be a 10 cm (4") cone-type woofer. The high frequency component shall be a balanced dome tweeter. For clear, wide-area sound coverage, the speaker shall 90° (H) x 90° (V) wide dispersion-angle high frequency horn.
The speaker shall come with separate HF and LF protection circuitry.
The speaker shall be rated at 8 ohms. The sensitivity at a distance of 1m with a 1 W input level applied shall be 87 dB. The rated power handling shall be 30 W continuous pink noise and 90 W continuous program. The speaker shall have a frequency response of 85 – 20kHz.
The speaker enclosure shall be constructed of HIPS resin. The speaker shall be available in white or black, and also be repaintable. The grille shall be a punched net, surface-treated steel plate. Brackets for speaker stand, wall and ceiling installation shall be included. There shall be also optionally available brackets for more demanding installations.
The unit shall be compact and lightweight with dimensions of 130 x 202 x 131 mm (5.12" x 7.95" x 5.16") and a weight of 1.8 kg (3.97 lbs.).

The speaker shall be a TOA model F-1000B/F-1000W. 
The board hanger bracket shall be the HY-BH10B. 
The ceiling mount bracket shall be the HY-CM10B/HY-CM10W.
The cluster bracket shall be the HY-CL10B.