Product program / Loudspeaker / Wall

F-1300BT

The speaker shall be a two-way bass reflex enclosure suitable for ceiling or wall mounting. The low frequency component shall be a 13 cm (5") cone-type woofer. The high frequency component shall be a 25 mm (1") dome tweeter. For clear, wide-area sound coverage, the speaker shall be 110° (H) x 100° (V) wide dispersion angle high frequency horn.
The rated input shall be 30 W. The speaker shall include a transformer having multiple taps (1 W, 3 W, 10 W, 30 W at 100 V and 0.5 W, 1.5 W, 5 W, 15 W, 30 W at 70 V) adjustable via the rear of the enclosure. The sensitivity at a distance of 1 m with 1 W of input level applied shall be 90 dB. The speaker shall have a frequency response from 80 to 20k Hz.
The speaker enclosure shall be constructed of HIPS resin. The speaker shall be available in white or black, and also be repaintable. The grille shall be a surface treated steel plate. Brackets for speaker stand, wall and ceiling installation shall be included. There shall be also optionally available brackets for more demanding installations.
The unit shall be compact and lightweight with dimensions of 162 x 250 x 161 mm (6.38" x 9.84" x 6.34") and a weight of 3.6 kg (7.94 lbs.).

The speaker shall be a TOA model F-1300BT/F-1300WT.
The board hanger bracket shall be the HY-BH10B.
The ceiling mount bracket shall be the HY-CM10B/HY-CM10W.
The cluster bracket shall be the HY-CL10B.
The subwoofer shall be the FB-120B/120W.