Product program / Loudspeaker / Wall

F-1300WTWPEB-Q

Weatherproof, compact 2-way design speaker in an attractive housing made of impact-resistant polystyrene with steel mesh panel. The extremely stiff construction of the housing achieved by the housing material and its shape minimizes the resonance, thereby allowing a clear reproduction. Tweeter with octagon horn for improved sound dispersion characteristics compared to a standard CD horn. Rear rotary switch for power adjustment.
Including swivel and tilt wall / ceiling mount, which can be attached to the bottom and back of the speaker.

Rated power: 30 W

Tappings 100V:	30/10/3/1 Watt

Tappings 70V: 30/15/5/1,5/0,5 Watt

Frequency range: 80 - 20000 Hz (-10 dB)
SPL: 90 dB (1W, 1m)

Dispersion angle (-6 dB): 110 &deg; x 100 &deg;

Degree of protection: IPX4 

Type (EN 54-24):	A

Dimensions (W x H x D): 162 × 250 × 161 mm

Weight: 3.6 kg (incl. bracket)

Color: white

Brand: TOA

Type: F-1300WBTWPEB-Q

Number of certificate:	1138/CPD/0282

Number of notified body:	1138