Product program / Loudspeaker / Wall

F-2000BTWPEB-Q

Weatherproof, compact 2-way design speaker in an attractive housing made of impact-resistant polystyrene with steel mesh panel. The extremely stiff construction of the housing achieved by the housing material and its shape minimizes the resonance, thereby allowing a clear reproduction. Tweeter with octagon horn for improved sound dispersion characteristics compared to a standard CD horn. Rear rotary switch for power adjustment.
Including swivel and tilt wall / ceiling mount, which can be attached to the bottom and back of the speaker.

Rated power: 60 W
Tappings 100V:	60/30/15/3 W

Tappings 70V: 60/30/15/7,5/1,5 W

Frequency range: 65 - 20000 Hz (-10 dB)

SPL: 92 dB (1W, 1m)

Dispersion angle (-6 dB): 110 ° x 100 ° (with Hornadapter: 80° × 80°)

Degree of protection:
 IPX4 
Type (EN 54-24):	A

Dimensions (W x H x D): 244 × 373 × 235 mm

Weight: 7.4 kg (incl. bracket)

Color: black

Brand: TOA
Type: F-2000BTWPEB-Q

Number of certificate:	1138/CPD/0282

Number of notified body:	1138