Product program / Loudspeaker / Wall

F-2000BT

The speaker shall be a two-way bass reflex enclosure suitable for ceiling or wall mounting. The low frequency component shall be a 20 cm (8") cone-type woofer. The high frequency component shall be a 25 mm (1") dome tweeter. For clear, wide-area sound coverage, the speaker shall include 110&deg; (H) x 100&deg; (V) wide dispersion-angle high frequency horn, plus an easily added 80&deg; (H) x 80&deg; (V) dispersion angle horn adapter for tighter dispersion control.
The rated input shall be 60 W. The speaker shall include a transformer having multiple taps (3 W, 15 W, 30 W, 60 W at 100 V and 1.5 W, 7.5 W, 15 W, 30 W, 60 W at 70 V) adjustable via the rear of the enclosure. The sensitivity at a distance of 1m with 1 W input level applied shall be 92 dB and 93 dB using the horn adapter. The speaker shall have a frequency response of 65 – 20kHz.
The speaker enclosure shall be constructed of HIPS resin. The speaker shall be available in white or black, and also be repaintable. The grille shall be a punched net, surface-treated steel plate. Brackets for speakerstand, wall and ceiling installation shall be included, and there shall be also optionally available brackets for more demanding installation venues.
The unit shall be compact and lightweight with dimensions of 244 x 373 x 235 mm (9.61" x 14.69" x 9.25") and a weight of 7.4 kg (16.31 lbs.).

The speaker shall be TOA model F-2000BT/F-2000WT.
The ceiling mount bracket shall be the HY-CM20B/HY-CM20W.
The cluster bracket shall be the HY-CL20B.
The subwoofer shall be the FB-100 or FB-120B/W.