Product program / Loudspeaker / Subwoofer

FB-120W   EU

The sub bass loudspeaker systems shall incorporate a single 30 cm(12") transducer. System frequency response shall vary no more than +/-3 dB from 40 Hz to 1.2 kHz measured on axis. The loudspeaker shall produce a Sound Pressure Level (SPL) of 90 dB on axis at 1 meter with a power input of 1 Watt, and shall be capable of producing 600 watts of continuous power and have a nominal impedance of 8 Ohms.
The loudspeaker enclosure shall be rectangular in shape and will be of a plywood construction with punch net steel perforated front grill. It shall be finished in white.
Input connectors shall be Neutrik NL4 MP and two M4 terminal strips.