Product program / Loudspeaker / Garden

GS-302    EU

The speaker shall be a compact garden speaker ideal for paging and background music broadcast in such places like gardens, theme parks and resort facilities. Corrosion resistant material is adapted to the speaker exterior, ensuring prolonged use of the speaker in a water-splashed environment. The speaker shall comply with IEC IP-X4. The appearance of the garden speaker is design so to incorporate with the surrounding environment.

The speaker shall include a 12cm splash proof cone driver and built-in 100V line matching transformer with 30W, 15W, 10W, 5W and 3W taps. Sensitivity shall be 87 dB SPL (1 W / 1 m) and frequency response shall be 100 to 8k Hz. The speaker shall be operable within the temperature range of -10°C to + 50°C (14° F to +140° F).

The splash-resistant garden speaker shall be TOA model GS-302.