Product program / Loudspeaker / Box

HS-150W

The speaker shall be the two-way speaker with a sealed box enclosure with polypropylene and a protective punched front grill with a surface-treated steel plate. The continuous pink noise shall be 100 W at 8 ohms and continuous program power rating of 300 W at 8 ohms. The speaker shall feature a 38 cm (15”) woofer and a 6-balanced-dome tweeters array with a 90&deg; x 40&deg; dispersion. Frequency response shall be 70 to 20k Hz, with crossover at 3k Hz. Sensitivity shall be rated at 98 dB (1 W, 1 m). The speaker system shall be designed for both fixed installation uses and on-the-road and shall be capable of being easily carried with an accessory handle. Its built-in overload protection circuitry for tweeter shall cut off a signal when an excessive input signal is received. Input connections shall be via a speakon connector or screw terminal.
The speaker system shall weigh 12 kg and shall have dimensions of 451(W) x 560(H) x 400(D) mm. The operating temperature range shall be between -10&deg;C and +50&deg;C. The speakers shall be easily mounted in vertical or horizontal positions, with a wide range of optional brackets.
The two-way speaker system shall be a TOA model HS-150B/HS-150W or approved equivalent.
The wall/ceiling-mount bracket shall be TOA model HY-1500HB/HY-1500HW/HY-1500VB/HY-1500VW.
The ceiling-mount bracket used in conjunction with HY-1500HB/HY-1500HW/HY-1500VB/HY-1500VW shall be TOA model HY-C0801/ HY-C0801W.
The wall-mount bracket used in conjunction with HY-1500HB/HY-1500HW/HY-1500VB/HY-1500VW shall be TOA model HY-W0801/HY-W0801W.