Product program / Loudspeaker / Variable Array

HX-5B-WP  EB-Q

<p class="MsoNormal">Weatherproof High-performance loudspeaker with adjustable CD dispersion. In 4 stages adjustable vertical beam angle between 15 ° and 60 °, sound bundling (Beam angle) with free installation above 800 Hz, with flush wall or ceiling installation effective from 400 Hz. Due to coherent sound radiation no disturbing Interference (comb filter effects) for wall or ceiling mounting as well as vertical Assembly of two systems. With two Speakon connectors and a screw terminal connection. Including wall mounting and eyelets for Mounting the speaker on steel cables. Extensive optional accessories for Wall / ceiling and tripod mounting as well as combination with matching subwoofer. Ball-proof according to DIN 18032, Part 3.

&lt;/ p&gt;</p>
<p class="MsoNormal">Transmission range: 60 Hz - 20 kHz (-10 dB)

Rated power: 600 W

Horizontal beam angle: 100 °

Vertical beam angle: 15 °, 30 °, 45 °, 60 ° adjustable Sound pressure (1W, 1m):

98 dB (15 ° vert. disp angle.) <span>, &lt;/ span&gt; 97 dB (30 ° vert. disp.angle),

96 dB (45 ° vert. disp. angle.) <span>,

&lt;/ span&gt; 95 dB (60 ° vert. disp.angle) &lt;/ p&gt;</span></span></p>
<p class="MsoNormal"><span>Equipment: 4 woofers, 12 BDT tweeter

Degree of protection: IPx4

Color: black

Version: Polypropylene Foamed

Dimensions (W x H x D): 408 x 546 x 342 mm

Weight: 18 kg

&lt;/ p&gt;</span></p>
<p class="MsoNormal"><span>Brand: TOA

Type: HX-5B-WP EB-Q &lt;/ p&gt;</span></p>
<p class="MsoNormal"/>
<p class="MsoNormal"/>