Product program / Network Audio / IP Speaker

IP-A1PC238

IP ceiling speaker 8 W

The IP ceiling speaker shall be integrable into SIP environments via the open SIP protocol (according to RFC3261) and into VMS using the ONVIF® Profile S audio backchannel. Furthermore, the speaker shall be addressable via multicast, providing 20 slots for listening addresses, and via HTTP commands using its remote API (Application Programming Interface).

The IP speaker shall provide an internal storage for up to 20 audio files accepting the WAV and MP3 format. Up to 20 patterns shall be programmable for audio file activation including adjustable repeat intervals, play count setting, duration setting and timer functionality.

All device settings shall be executable through a browser interface and in addition, a free-of-charge setting software for adjusting the network setting of a group of IP speakers simultaneously shall be available.

The IP speaker shall receive its power supply over the network connection using PoE.

2 control inputs for activation of playback patterns, speaker mute or initiation of SIP calls (up to 2 destinations) shall be accessible via a removable terminal plug. 1 control output for triggering local devices shall also be included.

3 spring clamps and a safety wire attachment hole shall support an easy and safe installation.

Power source: PoE (IEEE802.3af Class 3)

Amplifier rated output: 8 W

Sensitivity: 94 dB (1 W, 1 m, 500 Hz - 5 kHz, pink noise)

Max. SPL: 103 dB (8 W, 1 m)

Frequency response: 60 Hz - 20 kHz (peak -20 dB)

Speaker component: 16 cm cone-type

Audio codecs: PCMU (G.711u), PCMA (G.711a), G.722

Network I/F: 100BASE-TX, Auto MDI/MDI-X, RJ45 connector

Network Protocol: TCP/IP, UDP, HTTP, RTP, RSTP, ARP, ICMP, IGMPv3, NTP,  SIP (RFC3261)

Control input: 2 channels, no-voltage make contact input

Control output: 1 channel, open collector output

Finish: Steel plate (frame), steel net (grill), white (RAL 9016 equivalent), paint

Dimensions (⌀xD): 230 mm x 89 mm

Weight: 880 g

Manufacturer: TOA

Product: IP-A1PC238