Product program / Network Audio / IP Station

IP-A1RM     Y

IP remote microphone

The IP remote microphone shall be integrable into SIP environments via the open SIP protocol (according to RFC3261). Furthermore, it shall be addressable via HTTP commands, using its remote API (Application Programming Interface). The device shall be able to perform SIP calls and multicast paging using a built-in microphone, an analogue AUX input, audio files uploaded by the installer, or an audio file recorded by the user.
In addition, it shall provide the possibility to store and send at least 10 different HTTP command sets, consisting of at least 20 commands each, and to perform a system mute which disables all compatible IP audio devices in the network.
The IP remote microphone shall provide an internal storage for at least 20 audio files accepting at least the WAV and MP3 format. At least 1 additional file shall be recordable manually using a built-in microphone. At least 20 patterns shall be programmable for audio file activation including adjustable repeat intervals, play count setting and duration setting.
All device settings shall be executable through a browser interface and in addition, a free-of-charge setting software for adjusting the network setting of a group of IP devices simultaneously shall be available.
The device shall provide an LCD including the possibility to access at least 50 virtual buttons with free function assignment for SIP calls, multicast paging, pattern activation, HTTP command transmission and control output activation, to display device information regarding network configuration and SIP configuration, and to perform settings for the display.
The IP remote microphone shall provide access to a scheduler function via web interface including a separate user access level without device configuration authority. The installation of a scheduler software shall not be required.
The IP remote microphone shall receive its power supply over the network connection using PoE.

Power source: PoE (IEEE802.3af Class 3)
Audio codecs: At least PCMU (G.711u), PCMA (G.711a), G.722
Network I/F: At least 100BASE-TX, Auto MDI/MDI-X, 1x RJ45 connector
Network protocol: At least TCP/IP, UDP, HTTP, RTP, RSTP, ARP, ICMP, NTP, SIP (RFC3261)
Microphone type: Unidirectional electret condenser microphone with indicator and volume control
Monitor speaker: Cone-type speaker, speaker volume adjustable, rated output: at least 1 W
AUX input: At least 1x line/mic (pad function: -20 dB, volume adjustable, 3.5 mm mini jack)
Control input: At least 2x no-voltage make contact input
Mute control input: At least 1x 24 V DC cut signal
Control output: At least 1x open collector output
LCD: At least 3“, 255 x 160 dots, with backlight
Finish: ABS resin, black, paint
Dimensions (WxHxD): 224 mm x 47.2 mm x 136 mm or less
Weight: 630 g or less

Manufacturer: TOA
Product: IP-A1RM