Product program / Network Audio / IP Speaker

IP-A1SC15

IP horn speaker 15 W

The IP horn speaker shall be integrable into SIP environments via the open SIP protocol (according to RFC3261) and into VMS using the ONVIF® Profile S audio backchannel. Furthermore, the speaker shall be addressable via multicast, providing 20 slots for listening addresses, and via HTTP commands using its remote API (Application Programming Interface).

The IP speaker shall provide an internal storage for up to 20 audio files accepting the WAV and MP3 format. Up to 20 patterns shall be programmable for audio file activation including adjustable repeat intervals, play count setting, duration setting and timer functionality.

All device settings shall be executable through a browser interface and in addition, a free-of-charge setting software for adjusting the network setting of a group of IP speakers simultaneously shall be available.

The IP speaker shall receive its power supply over the network connection using PoE+ or PoE.

2 control inputs for activation of playback patterns, speaker mute or initiation of SIP calls (up to 2 destinations) shall be accessible via a removable terminal plug. 1 control output for triggering local devices shall also be included.

The IP horn loudspeaker shall operate in temperature conditions of between -30 to + 55 &deg;C and provide a waterproof, IP66-compliant enclosure. A safety wire attachment ring shall support a safe installation.

Power source: PoE+ (IEEE802.3at Class 4), PoE (IEEE802.3af Class 3)

Amplifier rated output: 15 W

Sensitivity: 112 dB (1 W, 1 m, 500 Hz - 5 kHz, peak level)

Max. SPL: 124 dB (15 W, 1 m) (1 W, 1 m, 500 Hz - 5 kHz, peak level)

Frequency response: 280 Hz – 12.5 kHz

Audio codecs: PCMU (G.711u), PCMA (G.711a), G.722

Network I/F: 100BASE-TX, Auto MDI/MDI-X, RJ45 connector

Network Protocol: TCP/IP, UDP, HTTP, RTP, RSTP, ARP, ICMP, IGMPv3, NTP, SIP (RFC3261)

Control input: 2 channels, no-voltage make contact input

Control output: 1 channel, open collector output

Dust/Water protection: IP66

Finish: [Horn flare, body] Aluminium, off-white (RAL 9010 equivalent), paint
&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp; [Reflector horn] ABS resin, off-white (RAL 9010 equivalent)
&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp; [Rear cover] PC resin, off-white (RAL 9010 equivalent), paint
&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp; [Bracket, screws and bolts] Stainless steel

Dimensions (WxDxH): 222 mm x 211 mm x 276 mm

Weight: 1.4 kg

Manufacturer: TOA

Product: IP-A1SC15