Product program / Wireless / Accessory

IR-200BC  CE

There shall be an available “table-top” charging station housed in an ABS plastic case which shall have dimensions of 9.4” (W) x 4.3” (H) x 3.9” (D) and weigh 1.4 lbs. The unit shall have two top-oriented charging bays to accommodate either the IR-200M or IR-300M (with a supplied adapter). The unit shall be powered via a 24VDC power adapter and shall consume a max of 2A.
The unit shall be called the TOA IR-200BC.