Product program / Wireless / Beltpack

IR-300M   Y

The pendent-style transmitter model shall be housed in an ABS plastic case measuring 2.5” (W) x 3.6” (H) x 1.1” (D) &amp;&nbsp; weighing .3lbs (incl. batteries &amp; strap). It shall include an integrated omni-directional microphone and also an input for use with an external lapel or headset mic via a 3.5mm mini-jack. There shall be an array of multiple IR LEDs at the front of the housing to facilitate clear transmission. There shall be an internal switch for selecting sensitivity for use with different external microphones. The unit shall have a frequency response of 100Hz to 12kHz and can accept a maximum Sound Pressure Level of 120dB. The unit shall be treated with an anti-bacterial coating to help reduce the likelihood of transmitting common bacterial agents from user to user. An integrated nylon lanyard allows the pendent to be comfortably worn around the user’s neck.
The unit shall be called the TOA IR-300M.