Product program / Wireless / Receiver / Module

IR-500R   Y

The wall-mount receiver shall be housed on a metal back plate and fitted with a dark tinted plexiglass cover with overall dimensions of 3.0” (W) x 4.7” (H) x 2.8” (D) and weighing .5 lbs. The unit shall have a BNC-type jack for connection to the IR-702T Tuner from which it will also receive 24VDC power. The receiver shall be capable of being installed in a single-gang electrical circuit box and is equipped with power indicator LED. The receiver shall have a reception area of up to approximately 49' line of sight and shall have an internally adjustable infrared light reception angle of between 50&deg; &amp; 80&deg; both horizontally &amp; vertically. The receiver shall also include a wall-mounting bracket. The unit shall be called the TOA IR-500R.