Product program / Wireless / Receiver / Module

IR-510R   Y

The ceiling-mount receiver shall be housed on a circular metal back plate and fitted with a dark tinted plexiglass dome cover with overall dimensions of 4 .7 ” (W) x 2.8” (H) x 0.5” (D) and weighing .5 lbs. The unit shall have a BNCtype jack for connection to the IR-702T tuner from which it will also receive 24VDC power and shall be equipped with power indicator LED. The receiver shall have a reception radius of up to approximately 26' line of sight and a coverage angle of 360&deg;. The unit shall be called the TOA IR-510R.