Product program / Wireless / Receiver / Module

IR-520R   Y

The stand-mount receiver shall be housed on a rectangular metal back plate and fitted with a dark tinted plexi-glass dome cover with overall dimensions of 33 .3” (W) 2.5” (H) x 1.3” (D) and weighing .2 lbs. The unit shall have a BNC type jack for connection to the IR-702T tuner from which it will also receive 24VDC power and shall be equipped with power indicator LED. The receiver shall have a reception area of up to approximately 49' line of sight. The unit shall be called the TOA IR-520R.