Product program / Wireless / Antenna distributor

IR-700D   CE

There shall be an available active IR receiver distributor for allowing expansion of the number of IR receivers in larger spaces. The unit shall be housed in a 1U ½ rack case, with dimensions of 8.3” (W) x 1.7” (H) x 7.9” (D) and weighing 1.4 lbs and shall be capable of being rack mounted with an optional kit (MB-WT3/MB-WT4). The unit shall be equipped with (4) 75 ohm BNC-type receiver mixing inputs and (2) 75 ohm BNC-type distribution outputs. The unit shall allow for use of up to 16 IR receivers in any combination when used in conjunction with the IR-702T and up to four passive distributor adaptors (models YW-1022/1024). The unit shall be powered by a supplied 24VDC external power adapter and shall consume a max of 25W. 
The unit shall be called the TOA IR-700D.