Product program / System Component / I/O Modules

M-01F

The microphone input module shall be balanced, 200 ohms with low/hi-cut filters and female XLR connector.

The microphone input module shall be TOA model M-01F.