Product program / Mixer / Processor Unit

M-66      CE

<p class="MsoNormal"><span lang="EN">Signal mixing and
distribution unit, featuring split function and mix function. Separately
switchable function for each channel, microphone preamplifier (up to 6 units) enable
different combinations of mixing and distribution. 6 balanced </span><span title="Eingänge mit Verstärkungsumschaltung (MIC: 60 dB, LINE: 10 dB) und Dämpfungsschalter (PAD: 20dB), Mischeingang, Verteileingang mit Dämpfungsschalter (PAD: 20dB), 6 symmetrische Direkt-/Verteilausgänge, Misch- und Brückenausgang zur Kaskadierung mehrerer Signalmisch- und">Inputs
with gain switching (MIC: 60 dB, LINE: 10 dB) and attenuation switch (PAD:
20dB), mixing input, distribution input with attenuation switch (PAD: 20dB), 6
balanced direct / distribution outputs, mixing and bridge output for cascading
several signal mixing and switching outputs </span><span title="-verteileinheiten. ">– and distribution.
</span><span title="Plexiglasabdeckung für die Front des Gerätes zum Schutz vor versehentlichem oder unbefugtem Verstellen der Parameter, XLR-Buchsen für Ein- und Ausgänge, 19&amp;#34;-Gehäuse mit 2 HE  ">Acrylic
glass cover for the front of the device to prevent accidental or unauthorized
adjustment of parameters, XLR sockets for inputs and outputs, 19 " x 2 units
housing

</span><span lang="EN-US"/><span title="Empfindlichkeit MIC/LINE: -60/-10 dBV (+20 dB mit PAD) ">Sensitivity
MIC / LINE: <span>&nbsp; </span>-60 / -10 dBV (+20 dB with
PAD)
</span><span title="Empfindlichkeit Line-Eingang: -10 dBV ">Sensitivity
line input:<span>&nbsp;&nbsp;&nbsp;&nbsp; </span> -10 dBV
</span><span title="Empfindlichkeit Split-Eingang: -10 dBV ">Sensitivity
split input: <span>&nbsp;&nbsp; </span>-10 dBV
</span><span title="Empfindlichkeit Mixeingang: +4 dBV ">Sensitivity
mix input: <span>&nbsp;&nbsp;&nbsp; </span>+4 dBV
</span><span title="Nennausgangspegel: +4 dBV ">Rated output level: <span>&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp; </span>+4 dBV
</span><span title="Übertragungsbereich: 20 - 20.000 Hz ">Transmission
range:<span>&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp; </span> 20 - 20,000 Hz
</span><span title="Klirrfaktor:  &lt; 0,01%  ">THD:<span>&nbsp;&nbsp;&nbsp;&nbsp;&nbsp; </span> &lt;0.01%
</span><span lang="EN">
</span><span title="Fabrikat: TOA ">Brand: TOA
</span><span title="Typ: M-66">Type: M-66</span></p>