Product program / Mixer / Accessory

M-800DT-EB

Dante Module

The module shall be insertable into the M-8080D matrix mixer by TOA Electronics. It shall support a port speed of 100/1000 Mbps with DHCP functionality. The module shall provide at least 8 Dante channels for bidirectional digital streaming. It shall feature multiple indicators to display the status.

- Power Source: 5 V DV

- Digital Audio Formats: TDM

- Audio Transport Formats: Dante Audio over IP

- Operating Temperature: 0 °C or less to 40 °C or more

- Operating Humidity: 90 %RH or more

- Finish: Panel: Surface-treated steel plate, black, paint

- Dimensions: 122.2 (W) x 33.5 (H) x 119.5 (D) or less

- Weight: 118 g or less

Manufacturer: TOA

Product: M-800DT