Product program / Mixer / Accessory

M-800RCT-EB

Wall mount touch LC-Display volume controller

The remote controller shall be compatible with TOA's M-8080D matrix mixer. The device shall have a display with a size of at least 4.3”. The display shall show the volume and the signal level for a dedicated output, the ID and communication status. It shall also be able to route any input to any output of the matrix mixer. The product shall be wall mountable. The GUI of the device shall let the user set the volume of dedicated channels using a digital fader. It also shall have a mute function, and an indicator shall display the communication status &amp; ID number. A “menu” button shall bring the user back to the main page. It shall be possible to select specific presets and load them from the matrix mixer. It shall be possible to lock the device with a password.

- The product shall have a screen saver function.

- Power Source: 24 V

- Operating Humidity: 90 %RH or less

- Operating temperature: 0 °C or less to 40 °C or more

- Finish: Panel: Polycarbonate + ABS, white

- Dimensions: 150 (W) x 115 (H) x 28 (D) mm or less

- Weight: 0.28 kg or less

Manufacturer: TOA

Product: M-800RCT