Product program / System Microphone / Remote Microphone / Stations

M-800RM-EB

Paging Microphone

The paging microphone shall be capable of addressing at least 12 different zones. The device shall feature an LC display that shows the selected zones, volume, and ID number. It shall include signal status indicators that display the presence of a signal when the microphone is transmitting. Additionally, an LED shall indicate if the signal is clipping. Furthermore, the product shall have a communication status indicator to confirm when the connection is functioning properly. The microphone shall include volume control and zone selector knobs. It shall feature a dedicated button for selecting all available zones simultaneously. A push-to-talk button shall initiate the microphone signal transmission, with an LED indicating its activation. A female 3-pin XLR connector shall be provided for connecting the microphone. The microphone shall also have a USB port to load WAV and MP3 files for chime sounds. The maximum chime duration shall be at least 4 seconds.

- Power Source: 24V DC (Powered by M-8080D or M-804EX)

- Audio Output: Electronic balanced, RJ45 Connector

- Gooseneck Microphone: Unidirectional electret condenser microphone

- Frequency Response: 20 or less – 20,000 Hz or more

- Total Harmonic Distortion: 0.01% or less

- Operating Temperature: 0°C to +40°C or less

- Operating Humidity: 90% RH or less

- Finish: Case: Surface-treated steel plate, black, paint

- Dimensions: 176 (W) x 61.8 (H) x 162.4 (D) mm or less

- Weight: 0.8 kg or less

Manufacturer: TOA

Product: M-800RM-EB