Product program / Mixer / Accessory

M-802RC-EB

Volume Controller

The volume controller shall be assignable to TOA’s M-8080D matrix mixer. It shall have the capability to adjust the output volume of different channels and route both input and output channels of the matrix mixer. The controller shall be equipped with an LCD display that shows the volume level, signal level for a designated output, ID, and communication status. Additionally, the device shall feature a rotary knob to set the volume and route the channels. The product shall have at least two analog outputs.

- Power Source: 24V DC

- Audio Output: Line output: 0 dBV, 20 dBu or more, electronic balanced, screw terminal (3 pins)

- Operating Temperature: 0°C or less to +40°C or more

- Operating Humidity: 90% RH or less

- Finish Panel: Polycarbonate + ABS, white

- Dimensions: 147 (W) x 86 (H) x 65 (D) mm or less

- Weight: 0.3 kg or less

Manufacturer: TOA

Product: M-802RC