Product program / Mixer / Mixer Unit

M-8080D-EB

8x8 DIGITAL MATRIX MIXER 

The digital matrix mixer shall offer 8 analogue audio inputs and 8 audio outputs.

It shall be expandable to a maximum number of 12x audio in-/12x audio outputs via optional remote devices of the 8X8 DIGITAL MATRIX MIXER Series with audio in / audio output function.

An LCD shall display name, preset, Firmware Version and connection status. Each Input/Output must indicate a present signal / clipping signal.

It shall be ready to connect remote controllers and/or remote controllers with audio input and/or audio output terminals and/or remote paging microphones of the Series.

It shall be possible to install an optional dante modul to connect up to 16 different M-8080D with each other.
An ethernet interface (DHCP) for remote PC configuration and control shall be available.

The configuration of the detailed system setting and the storage of the configuration data shall be possible via PC Software.

The cabling between the digital matrix mixer and the remote devices shall be Cat5e cables.

The digital matrix mixer shall be compact size (1HU) and shall be ready for 19“ rackmount.

The digital matrix mixer shall offer following DSP functions for the Audio Inputs:

Ducker, Gain, Gate, Expander, 5 band EQ, Delay, Limiter/Compressor.

The digital matrix mixer shall offer following DSP functions for the audio outputs:

Mixer, Crossover, Gain/Phase, 8 band EQ, Delay, Limiter / compressor.

It shall support Ducker function (Input priority), Feedback Compression, Auto Mixer.

Configuration files and Presets must be configurable and exportable to PC.

8x8 DIGITAL MATRIX MIXER Series consist of: 8x8 DIGITAL MATRIX MIXER, REMOTE AUDIO CONTROL PANEL, REMOTE AUDIO CONTROL PANEL WITH AUDIO OUT, REMOTE AUDIO CONTROL PANEL WITH TOUCH DISPLAY, REMOTE AUDIO INPUT OUTPUT PANEL, REMOTE MICROPHONE, EXTENSION MODULE 4 PORTS