Product program / Mixer / Mixer Unit

M-8080D-EB

Digital Matrix Mixer

The mixer shall conform to a 19-inch standard rack size with a height of 1U. The digital matrix mixer shall have a minimum of 8 analog input and output channels, with the capability to expand to at least 12 channels through the addition of peripheral devices. The mixer shall have an interface for a Dante card, which shall enable the mixer to become a Dante-capable device. It shall be possible to interconnect multiple mixers using Dante to extend the number of channels to at least 192 inputs and outputs. The mixer shall feature a relay port on the rear panel, where the on/off status can be individually controlled via the system menu. These relays shall be generally used as switches for third-party electrical equipment. The mixer shall include an input priority function, a mute-all-outputs function, and an emergency priority function, all of which shall be triggered by an external signal connectable to at least two ports on the rear of the device. For connecting the device to PC software, it shall be equipped with a LAN port, including a switch to enable or disable the port. The software shall provide a setup page for the following DSP functions: 8-band Equalizer, Gate, Compressor, Ducker, Feedback suppression, Auto Mixer, and Delay. The front panel of the device shall have an LC display showing the device name, firmware version, preset, and ID number. The device shall also feature LEDs indicating signal clipping, malfunctions, communication status, and power. The mixer shall support several peripheral devices, which shall be configurable through the software. The following remote devices shall be available: paging microphone, audio input and output modules providing at least 2 analog channels in and 2 analog channels out, volume controller, and a touch LC display for controlling volume and routing. The device shall have at least two ports on the rear panel for connecting these modules. The minimum working range for these modules shall be 100 meters, depending on the CAT cable used. A software application for Windows shall be available for controlling and setting up the device.

Power Source: 100 – 240 V AC, 50/60 Hz

Power Consumption: 40 W or less

Audio Input: - 48 dBV or less to 0 dBV, electronically balanced, removable terminal block (3 pins)

Audio Output: 0 dBV, electronically balanced, removable terminal block (3 pins)

Frequency Response: 20 or less – 20000 Hz or more

Total Harmonic Distortion: 0.01 % or less

S/N Ratio: 105 dB or more

Crosstalk: 79 dB or more

Phantom Power: +48 VDC, switchable

Equalizer/Filter: 5 band EQ for in and 8 band EQ for out

A/D Converter: 24 bits

Sampling Frequency: 48 kHz

Operating Temperature: 0 °C or less to + 40 °C or more

Operating Humidity: 90 % RH or less

Finish: Panel: Aluminum, black / Case: Surface-treated steel plate, black, paint

Weight: 4.58 kg or less

Manufacturer: TOA

Product: M-8080D-EB