Product program / Mixer / Accessory

M-822IO-EB

Remote Audio Input and Output Controller

The remote controller shall be compatible with TOA's M-8080D matrix mixer. It shall provide 2 analog input channels and 2 analog output channels. The device shall include an XLR microphone input. The input level of the microphone shall be adjustable via a knob. The device shall be equipped with a switch to enable or disable the phantom power function (48V) for an electret microphone. Indicators shall display the status for signal presence and clipping.

- Power Source: 24 V DC

- Audio Input: Mic Input: - 48dB, electronic balanced, XLR Connector

- Audio Output: Line output: 0 dBV, output 20 dBu or more, electronic balanced, screw terminal (3 pins)

- Frequency Response: 20 or less to 20.0000 Hz or more

- Total Harmonic Distortion: 0.01 %

- S/N Ratio: 105 dB or more

- Crosstalk: 79 dB or more

- Operating Temperature: 0 °C or less to 40 °C or more

- Operating Humidity: 90 % RH or less

- Finish: Panel: Polycarbonate + ABS, white

- Dimensions: 147 (W) x 86 (H) x 63 (D) mm or less

- Weight: 0.3 kg or less

Manufacturer: TOA

Product: M-822IO