Product program / System Component / Audio Source

MD-210CTU-EB

The music device shall be a 1U 19" rack-sized all-in-one player. It shall be capable of playing various audio sources, such as CDs, USBs, SD/MMC Cards, and FM Radio. The option to select CD, USB, or SD/MMC as the audio source shall be available, while the tuner mode plays FM radio. The device shall be equipped with RCA audio outputs for both left (L) and right (R) channels for FM, CD/USB/SD, and priority audio. Furthermore, the device shall include a key that facilitates switching between CD mode and tuner mode. The FM radio tuner shall have the capacity to store up to at least 30 channels in its preset memory. Additionally, a sleep function lasting a minimum of 90 minutes shall be featured in tuner mode. Incorporating an A-B function, the device shall permit the looping of specific sequences. It shall also integrate a key that enables the repetition of selected tracks or folders. Moreover, the device shall provide the capability to play all tracks in a random manner. The device shall support the RDS standard communication protocokl. Additionally, the device shall include a switch allowing for the selection of Mono or Stereo mode.
<ul>
<li>Maximum 8 W</li>
<li>Frequency Response: Maximum 20 kHz - 20,000 Hz, ±3dB</li>
<li>Tuner Receiving Frequency: Maximum 87.5 MHz - Minimum 108 MHz (in 50 kHz steps)</li>
<li>Memory Tuner Channels: Minimum 30 Channels in total for FM broadcasts</li>
<li>Operating Temperature: Maximum 0°C - Minimum +40°C</li>
<li>Operating Humidity: Maximum 90% RH or lower</li>
<li>Dimensions: Maximum 482 (W) mm x 44 (H) Maximum mm x Maximum 250 (D) mm</li>
<li>Weight: Maximum 3.5 kg</li>
</ul>