Product program / Accessories / Monitor Panel

MP-1216   H

<span lang="EN">Control and monitor unit for 16 floating inputs, designed for 19 "rack installation requiring 2 units height. <span>&nbsp;</span>12-segment LED meter to display the level of each channel, scaling in dB and W. Built-in 3 W monitoring loudspeaker, automatic switchover to headphone when jack is plugged-in, volume control, detent endless turntable to select the monitoring channel, control panel cascadable to control more than 16 channels, while all channels can be monitored via one device, each channel matched to three different levels inputs</span>
<p class="MsoNormal"><span lang="EN"><span lang="EN">

Inputs: <span>16

Nominal level for display 0 dB: +4 dB (Line) / 49V (300W to 8 ohms) /100V (for 100V technology)

Display range:<span>&nbsp;&nbsp;</span> -30 dB to +6 dB / 0.3W to 1200W

Headphones: <span>&nbsp;&nbsp;</span> 6.3 mm jack, 10mW

Dimensions (W x H x D):&nbsp;<span>482.6 x 88.4 x 312.7 mm

Color:&nbsp; <span>Black

Brand: TOA

Type: MP-1216</span></span></span></span></span></p>