Product program / Amplifier / Mixer Amplifier

MX-6224D    1CE

<div>The digital mixer power amplifier will have 6 MIC inputs and 6 Outputs. It will operate on AC mains or from a 220V – 240V AC, 50/60Hz line.&nbsp; The amplifier shall meet the following performance criteria: Power consumption shall be 150W according to IEC60065 and 650W at rated output of both 2ch with less than 1% THD at 50Hz to 20kHz at 1/3 rated output, rated load, from power amplifier input. It shall be power amplifier class D. It will include 2 x 240 Watt digital amplifiers, allowing for internal and external zones. It will include 3 band EQ, which will be available on all 6 mic inputs, which will allow users to find preferable sound quality easily without the technical experience other EQ bands require. Three microphone inputs will have increased sensitivity to 6dBV allowing the speaker to move around the microphone freely. It shall include a built in digital amp and DSP module which will provide exceptional sound quality. The hardware will be simply designed and compact to install. An optional remote control panel will be available. The digital mixer power amplifier will have a high pass filter ensuring speakers are less vulnerable to damage. It’s built in speaker EQ will reduce acoustic feedback and ensure more intelligible sound. It will include a built in effector, realizing celestial sound in small buildings where lack of reverberation needs to be compensated for.&nbsp; The dimensions shall be 420 (W) X 99 (H) X 364.8 (D) mm and weight 6.5kg.</div><div>
</div><div>The amplifier shall be TOA model MX-6224D.</div>