Product program / Network Audio / I/F Unit

N-8000AL  CE

The telephone interface unit is designed for use with TOA's packet intercom system (IP network compatible intercom system) that employs the packet audio technology and can be connected to an existing local area network (LAN) or wide area network (WAN).
Network shall be made possible using RJ45 connection via a switching hub. Network interface shall be I/F 10BASE-T/100BASE-TX (Automatic-Negotiation) Auto MDI/MDI-X compatible Network Protocol TCP/IP, UDP, ARP, ICMP, HTTP, RTP, IGMP. 

The telephone interface unit shall have a single telephone socket allowing the connection of an analogue telephone, by connecting the telephone interface unit to a LAN via its RJ45 connector permits the analogue telephone to be operated in the same manner as an intercom master station.
The telephone interface unit shall have indication lamps on the front panel displaying: 
LNK/ACT lights green when connected to a network, and flashes while transmitting or receiving data. STATUS continuously lights red while data is written to an internal storage medium. POWER lights green when power is supplied to the unit. LINE INDICATOR lights green when the connected telephone is off-hook.
The telephone interface unit shall include dedicated software that will enable centralised control, log verification and system maintenance from a personal computer. Line supervision can also be performed using a personal computer and Internet browser.
Power requirements shall be 220 – 240V AC.
It shall use only one-half EIA component rack space and its dimensions shall be 210 (W) × 44.3 (H) × 267 (D) mm (8.27" × 1.74" × 10.51") Weight shall be 1.7 kg (3.75 lb.) and finished in black pre-coated steel plate. Alternatively, the unit can be free standing or wall mounted
Optional extras: MB-15B-BK rack mounting bracket (for rack mounting one unit). MB-15B-J rack mounting bracket (for rack mounting two units). YC-850 wall mounting bracket manufactured by TOA Corporation.