Product program / Network Audio / IP Exchange

N-8000EX  CE

Fully digital IP mediation unit with connections for 16 stations. 2 Audio outputs control output for announcements / control external audio equipment. Connection to other teaching units, universal interface and IP intercom stations on a network.
Connecting the stations in 2-wire technique. No separate power supply of needed receivers. 4 internal and 8 external communication channels are also available.
Programmable functions:
Call, announcements, speed dial, manual call forwarding, automatic call forwarding, time-based call routing, adjustable time limitation for discussions, announcements and ringtone, automatic activation of control outputs (E.g. call door intercom - activation CCTV via control output), automatic call activation control input, group call, call forwarding in "Occupied", Office - call forward unconditional (time adjustable), auto answer, classic answer, automatic direct dial at the receiver, priority call, choice of call priority, and message priority, choosing from up to 8 background music sources, adjustable microphone sensitivity and ringer volume speaker volume. 
Additional grouping with customizable access rights regarding call and announcement permissions of the groups themselves.
3 Status LED indicators for: operation, status and network.
Including system software for Windows®2000 / Windows®XP.