Product program / Network Audio / I/F Unit

N-8000MI  CE-GB

Universal interface for connecting to external systems, 
configurable/programmable for:
-Announcements, activated 2 audio inputs for the supply of background music or control inputs
-2 Audio outputs for the transmission of announcements in external audio systems (E.g. PA systems),
-2 Connections to a telephone system with pulse or tone dialing,
-2 Leased line connections to EXES-2000 and 
EXES-6000 intercom systems,
-16 Control inputs for zone control for externally-powered announcements, dial-up, receiving a busy signal of an external audio system, switching on control output
-16 Control outputs: can be activated by a number of the stations and automatically when a call (E.g. to activate camera system), occupied and error display
Automatic system diagnosis (every 20 seconds) of receivers, teaching units, IP Intercoms and universal interface for network status, CPU error, synchronization problems and missing receivers.