Product program / Network Audio / IP Exchange

N-8010EX  CE

Fully digital IP mediation unit with connections for 16 stations. Connection to other teaching units, universal interface and IP intercom stations on a network. Connecting the stations in 2-wire technique. No separate power supply of needed receivers. 1 internal and 2 external communication channels are also available.
Programmable functions:
Call, announcements, speed dial, manual call forwarding, automatic call forwarding, time-based call routing, adjustable time limitation for discussions, announcements and ringtone, automatic activation of control outputs (E.g. call door intercom - CCTV via contact output activation), automatic call activation control input, group call, call forwarding to "Busy", Office - call forward unconditional (time adjustable), auto answer, classic answer, automatic direct dial at the receiver, priority call, choosing from up to 8 sources of background music, adjustable microphone sensitivity, ringer volume, speaker volume. 
Additional grouping with customizable access rights regarding call and announcement permissions of the groups themselves.
3 Status LED indicators for: operation, status, network.
Including system software for Windows®2000 / Windows®XP.