Product program / System Microphone / Remote Microphone / Stations

N-8033MS  Y

The flush mount master station is designed for use with TOA's packet intercom system (IP network compatible intercom system) that employs the packet audio technology.
The master station is a 2-wire system and shall be capable of automatic duplex hands free operation without the use of handsets and shall employ echo cancellation. The master station shall have 4 control inputs to facilitate automatic call selection allowing the user to make calls via a contact such as a footswitch.
The master station shall also perform the following features: Voice calling, Automatic connection, Continuous call, One-touch dialing, Call hold, Automatic call forwarding, Emergency paging, Scan monitoring, Three-party conference and many more.
The unit shall have an IP65 ingress protection and shall be resistant to chemicals. The master station shall be capable of being flush mounted or surface mounted using an optional back box.
Dimension shall be 115 (W) × 254 (H) × 51 (D) mm (4.53” x 10” x 2.01”) weighing 850 g (1.87 lb.) and finished with a replaceable polyester film front membrane.
&nbsp;
Optional extras: YC-841 back box manufactured by TOA Corporation.